How to operate Upper Computer





**Step1**: Pls click below link to download driver:


<https://dalyelec.cn/daly/zytool.zip>


If can’t find it, pls try this link again to download:

<https://drive.google.com/file/d/1OXCHvjAHyVCa7Y1x8pk6tgl_bhVTnwkL/view?usp=sharing>


How to install this software:

1. 
2. 
3. 
4. 
5. 
6. 
7. 
8. Go to the disk which you saved just now to find the “exe”. And double click it.



1. 

**Step2**: Pls select correct options for red frames



**IC Name**:

If your BMS is **3-5S**, pls select: **SH39F003**

If your BMS is **6-10S**,pls select: **SH39F004**


**Comm PortNo**.:

Pls check your computer--Device Management--Serial Port Management--Check the COM port in your PC what it is, and select correct one. **Example: If it is COM1 so that pls select “COM1”**


**Baud Rate**: Pls select 9600

**Step3**: Click “OK”

**Step4**: Click” Scan All”, Like as below picture




**Step5**：Pls select MCU, then click “Read All”



If you didn’t tell us the capacity of your battery pack when you placed order, We would set a fake one for default. So you should change it. If you provided, and the data is right, no need change.

**Step6**: Change capacity of battery pack



Edited by Nimi of Daly